534 West 42nd Street 
Network Configuration  August 10, 2018
------Verizon---------
Purpose:  Our online Verizon account
Username: 534Agent  Password: 10036W42
------Verizon Router----
Purpose:  Provides internet connectivity and lan routing for Wally Sensor Monitoring, Honeywell WIFI Thermostats (Lobby and Basement), Amcrest IP Web Camera, Apple Mac Mini (for Tekmar Boiler Monitoring) and Amped Wireless Access Point
Physical Location:  Gas and Water Meter Room Left Wall Bottom Router
Dynamic IP Address
Remote Administration:   http://534w42.hopto.org:8080 
Username: claude  Password: carnival   (administrator)
Username:john  Password: jeff   (administrator)
Local IP Address: 192.168.1.1
DHCP IP Range: 192.168.1.121-254
WPA2 Security SSID: TTTK2  Wireless Password: TW5W6F3CRZ7QLQ7H
------Amped Wireless Access Point-------
Purpose: Extends the range of Verizon Router to provide internet access to devices listed above. It is connected to Verizon Router via ethernet cable.  It is a power over ethernet device.
Physical Location:  Left wall by washer dryer affixed to metal conduit
Static Ip Address: 192.168.1.2  Default Gateway: 192.168.1.1
Remote Administration: http://534w42.hopto.org:80 (standard http port)
Username: 534Agent  Password: W42wap534
WPA2 Security SSID: 534basementwap  Wireless Password: W42wap534
DHCP is disabled (DHCP is handled by Verizon Router).
It has an external antenna which is currently deactivated.

------Amcrest Webcam (Rear Basement)------------
Purpose:  To provide monitoring of the rear sump in case of a water signal
Physical Location: Rear of building on wall above rear sump
Static Ip Address:  192.168.1.120
MAC: 9c:8e:cd:15:f2:10
Remote Access: http://534w42.hopto.org:8000
Remote Access via mobile device:  Amcrest View Pro App
Remote Access via desktop computer: Download Amcrest Surveilance Pro
Username: admin  Password: W4210036

------Amcrest Webcam (Boiler Room)------------
Purpose:  To provide monitoring of the boiler room
Physical Location: On the wall behind the hot water heater
Static Ip Address:  192.168.1.?
MAC: ?
Remote Access: http://534w42.hopto.org:8000
Remote Access via mobile device:  Amcrest View Pro App
Remote Access via desktop computer: Download Amcrest Surveilance Pro
Username: admin  Password: W4210036

------Amcrest Webcam (Gas and Water Room)------------
Purpose:  To provide monitoring of the gas and water room
Physical Location: In the corner near the Verizon boxes towards the ceiling
Static Ip Address:  192.168.1.?
MAC: ?
Remote Access: http://534w42.hopto.org:8000
Remote Access via mobile device:  Amcrest View Pro App
Remote Access via desktop computer: Download Amcrest Surveilance Pro
Username: admin  Password: W4210036

--------------Apple Mac Mini------------------------
Purpose:  To act as webserver for Tekmar 483 Gateway which allows monitoring of the boiler.
Physical Location:  Boiler Room to the left of the boilers in the corner.
Static IP Address: 192.168.1.100
MAC: 00:16:cb:04:df:e7
Username: johndoe   Password: carnival
Remote Access VIA VNC Client: http://534w42.hopto.org:590 
	Password: carnival
Remote Access (Webserver for Tekmar Gateway): http://534w42.hopto.org:3000
	Username: claude Password: carnival
	Username: john Password: jeff

------------Tekmar 483 Gateway---------------
Purpose: To act as a gateway between Apple mac mini and Tekmar devices via TN4 connections to the devices. Currently the only device attached is the Tekmar 274 Boiler Control
Physical Location: Boiler room, left of boilers
---------------- Wally Home Monitoring System----------------
Purpose: To remotely monitor heat, temperature, humidity and open/closed condition of various sensors in the basement.  It consists of a HUB and currently 9 sensors.

--------------Wally Hub--------------------------------
Purpose: To act as a gateway device for 9 sensors
Physical Location: Basement on wall to the right of the washer dryer area (black box with usually an orange light)
Dynamic IP Address
MAC: 90:7a:f1:ee:c8:31

------------Honeywell Thermostats------------------
Purpose: To allow remote monitoring and setting of lobby and basement thermostats
Physical Locations:   1) Lobby 2) Basement across the hall from the sink
1) Lobby:   MAC:  00:d0:2d:57:56:d5  For information to re register if necessary go to the thermostat config menu
2) Basement: