TRICOT    KNITTING    DATA
Changes from WW1211/4:  1) 40-12 Nylon 6, Dull, Ashfar (Kapak) instead of 40-13 Nylon 6, Dull, Hyosung
2) Slackened approx. 7% for target wt. 3.0 oz/yd2  3) Change in racks from 2220 to 2025 racks/pc for 330 lbs/pc

DEVELOPMENT :    WW1211/5	STYLE : 	DATE : 05/08/09	

Machine > 32gg – 2 Bar – Tricot 	Machine Width > 168”	Greige Width > 168”	
Width Repeat >	Fabric Description > U.B.L.	Racks / Piece > 2025	
Machine 15 & 16 (gears)	End Use > Medical laminates		

Beam No >1(back)	Runner > 46”	Warping > ( 1340 ends on 42” wide spools ) x 4    Commercial	

Yarn >    40-12 NYLON 6, Dull, Ashfar (Kapak – Korean Manufacturer) (U)	

Threading >      SOLID	
                                                                                                                                 *BAR 1  CHAIN :   1 – 0 / 1 – 2 //

Beam No >2(front)	Runner > 75 ½”	Warping > ( 1340 ends on 42” wide spools ) x 4    Commercial	

Yarn >    40-12 NYLON 6, Dull, Ashfar (Kapak – Korean Manufacturer) (U)	

Threading >      SOLID	
                                                                                                                                 *BAR 2  CHAIN :   1 – 0 / 3 – 4 //

Beam No >3	Runner >	Warping >	

Yarn >	

Threading >	

Beam No >4	Runner >	Warping >	

Yarn >	

Threading >	

  Top (B) >  78                        Top (B)> 86	Quality  (per Rack) > 10”	
Take-Up {------ =9.98”/rk  Batching{------  =10.42”/rk	Courses  /  Repeat   > 2	
   Bot (A) >  86                        Bot (A)> 99	S P E E D   (rpm)    > 	
Comments: Target weight 3.0 oz/yd2 

	Date:  01/04/08

STYLE :  WW1211/5	GAUGE :  32gg	

Courses Per Repeat :  2
BAR 1	BAR 2					
(Back)	(Front)					
1 – 0	1 – 0					
1 – 2	3 – 4